Colorado Traffic League Monthly Simplex Test					8/11/2026
1900 hrs
3.989MHz LSB
146.52 MHz 2-meter

Repeat 3 times:  Calling the Colorado Section traffic net monthly Simplex Test 

This is (Call Sign in ITU Phonetics) serving as Net Control.  The Colorado Traffic League holds monthly tests on 3.989 MHz LSB and 146.52 MHz 2-meter FM simplex to test our equipment and ability to operate in emergencies or when there is a failure on the Colorado Connections repeater system.

After participating stations have checked in, please make any contacts you can on 146.52 MHz.  

	Please record the contact’s Call Sign, Name and Location.

	If you have difficulty transmitting your contacts to Net Control than please relay your 	contacts to another station participating in this test for transmission to Net Control.

	If you were unable to make any contracts on 146.52 MHz please report zero contracts 	to Net 	Control.

	After you have checked back in and transmitted any contacts you are dismissed.

	I will record all contracts for the log.

Participating stations in this test please check-in now.

For stations reporting back in Net Control will repeat and confirm contracts and dismiss station after reporting.

Closing

Thank you to all who participated in this monthly simplex test.

This is (Call Sign) Net Control for this month’s Colorado Traffic League simplex test closing this net  at LOCAL Date & Time and UTC Date & Time.

73, (Call Sign)

This Monthly Test must end before 19:30 hrs for the Columbine Net.



